(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "nwX287")
    (date "2023-07-07")
    (rev "2")
    (company "Necroware")
    (comment 1 "by Scorp")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./gerber")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "VCC")
  (net 3 "SQW")
  (net 4 "AD7")
  (net 5 "AD6")
  (net 6 "AD5")
  (net 7 "AD4")
  (net 8 "INT")
  (net 9 "AD3")
  (net 10 "RST")
  (net 11 "AD2")
  (net 12 "DS")
  (net 13 "AD1")
  (net 14 "AD0")
  (net 15 "RW")
  (net 16 "AS")
  (net 17 "CS")
  (net 18 "BC")
  (net 19 "X2")
  (net 20 "X1")
  (net 21 "CEO")
  (net 22 "CEI")
  (net 23 "VOUT")
  (net 24 "unconnected-(U2-X1-Pad2)")
  (net 25 "unconnected-(U2-X2-Pad3)")
  (net 26 "unconnected-(U2-BC-Pad20)")
  (footprint "Package_DIP:DIP-24_W15.24mm_Socket" (layer "F.Cu")
    (at 127 79.459001)
    (descr "24-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket")
    (property "Sheetfile" "nwX287.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 7.62 -2.33) (layer "F.SilkS") hide)
    (fp_text value "socket" (at 7.62 30.27) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 7.62 13.97) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "VOUT") (pinfunction "VOUT") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "unconnected-(U2-X1-Pad2)") (pinfunction "X1") (pintype "input+no_connect"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "unconnected-(U2-X2-Pad3)") (pinfunction "X2") (pintype "input+no_connect"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "AD0") (pinfunction "AD0") (pintype "input"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "AD1") (pinfunction "AD1") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "AD2") (pinfunction "AD2") (pintype "input"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "AD3") (pinfunction "AD3") (pintype "input"))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "AD4") (pinfunction "AD4") (pintype "input"))
    (pad "9" thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "AD5") (pinfunction "AD5") (pintype "input"))
    (pad "10" thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "AD6") (pinfunction "AD6") (pintype "input"))
    (pad "11" thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "AD7") (pinfunction "AD7") (pintype "input"))
    (pad "12" thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "13" thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "CS") (pinfunction "CS") (pintype "input"))
    (pad "14" thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "AS") (pinfunction "AS") (pintype "input"))
    (pad "15" thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "RW") (pinfunction "R/~{W}") (pintype "input"))
    (pad "16" thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "17" thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "DS") (pinfunction "DS") (pintype "input"))
    (pad "18" thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "RST") (pinfunction "~{RST}") (pintype "input"))
    (pad "19" thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "INT") (pinfunction "~{INT}") (pintype "input"))
    (pad "20" thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 26 "unconnected-(U2-BC-Pad20)") (pinfunction "BC") (pintype "input+no_connect"))
    (pad "21" thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "CEI") (pinfunction "~{CEI}") (pintype "input"))
    (pad "22" thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "CEO") (pinfunction "~{CEO}") (pintype "input"))
    (pad "23" thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "SQW") (pinfunction "SQW") (pintype "input"))
    (pad "24" thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "VCC") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-24_W15.24mm_Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "nwX287:BatteryHolder_CR1220" (layer "F.Cu")
    (at 134.62 98.425 180)
    (property "Sheetfile" "nwX287.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single-cell battery")
    (property "ki_keywords" "battery cell")
    (attr through_hole)
    (fp_text reference "BT1" (at -3.048 8.636) (layer "F.SilkS"))
    (fp_text value "CR1220" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 0 -3.6 180) (size 1.2 1.2) (drill 1.2) (layers "F&B.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 0 3.9 180) (size 1.2 1.2) (drill 1.2) (layers "F&B.Cu" "*.Mask"))
    (pad "1" smd rect (at 0 8 180) (size 2.3 4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "BC") (pinfunction "+") (pintype "passive"))
    (pad "2" smd rect (at 0 -8 180) (size 2.3 4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "-") (pintype "passive"))
  )
  (footprint "Crystal:Crystal_SMD_FrontierElectronics_FM206" (layer "B.Cu")
    (at 135.636 85.471)
    (descr "SMD Watch Crystal FrontierElectronics FM206 6.0mm length 1.9mm diameter http://www.chinafronter.com/wp-content/uploads/2013/12/FM206.pdf")
    (tags "['FM206']")
    (property "Sheetfile" "nwX287.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Three pin crystal, GND on pin 3")
    (property "ki_keywords" "quartz ceramic resonator oscillator")
    (attr smd)
    (fp_text reference "Y1" (at 0 -5.461 180) (layer "B.SilkS"))
    (fp_text value "32.768kHz 6pF" (at 2.794 -0.635 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -0.3 180) (layer "B.Fab"))
    (pad "1" smd rect (at -1.27 3.5) (size 1 1.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "X2") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 1.27 3.5) (size 1 1.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "X1") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 0 -3.05) (size 3 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_FrontierElectronics_FM206.wrl"
      (offset (xyz 0 0.2249999962 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm" (layer "B.Cu")
    (at 134.62 99.568 180)
    (descr "SOIC, 24 Pin (JEDEC MS-013AD, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_wide-rw/RW_24.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "nwX287.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 8.636) (layer "B.SilkS"))
    (fp_text value "bq4285" (at 0 -0.635 180) (layer "B.SilkS"))
    (fp_text user "bq3285" (at 0 1.27) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -4.65 6.985 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 23 "VOUT") (pinfunction "VOUT") (pintype "input"))
    (pad "2" smd roundrect (at -4.65 5.715 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 20 "X1") (pinfunction "X1") (pintype "input"))
    (pad "3" smd roundrect (at -4.65 4.445 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "X2") (pinfunction "X2") (pintype "input"))
    (pad "4" smd roundrect (at -4.65 3.175 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "AD0") (pinfunction "AD0") (pintype "input"))
    (pad "5" smd roundrect (at -4.65 1.905 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "AD1") (pinfunction "AD1") (pintype "input"))
    (pad "6" smd roundrect (at -4.65 0.635 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "AD2") (pinfunction "AD2") (pintype "input"))
    (pad "7" smd roundrect (at -4.65 -0.635 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "AD3") (pinfunction "AD3") (pintype "input"))
    (pad "8" smd roundrect (at -4.65 -1.905 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "AD4") (pinfunction "AD4") (pintype "input"))
    (pad "9" smd roundrect (at -4.65 -3.175 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "AD5") (pinfunction "AD5") (pintype "input"))
    (pad "10" smd roundrect (at -4.65 -4.445 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "AD6") (pinfunction "AD6") (pintype "input"))
    (pad "11" smd roundrect (at -4.65 -5.715 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "AD7") (pinfunction "AD7") (pintype "input"))
    (pad "12" smd roundrect (at -4.65 -6.985 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "13" smd roundrect (at 4.65 -6.985 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "CS") (pinfunction "CS") (pintype "input"))
    (pad "14" smd roundrect (at 4.65 -5.715 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "AS") (pinfunction "AS") (pintype "input"))
    (pad "15" smd roundrect (at 4.65 -4.445 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 15 "RW") (pinfunction "R/~{W}") (pintype "input"))
    (pad "16" smd roundrect (at 4.65 -3.175 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "17" smd roundrect (at 4.65 -1.905 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "DS") (pinfunction "DS") (pintype "input"))
    (pad "18" smd roundrect (at 4.65 -0.635 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "RST") (pinfunction "~{RST}") (pintype "input"))
    (pad "19" smd roundrect (at 4.65 0.635 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "INT") (pinfunction "~{INT}") (pintype "input"))
    (pad "20" smd roundrect (at 4.65 1.905 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "BC") (pinfunction "BC") (pintype "input"))
    (pad "21" smd roundrect (at 4.65 3.175 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "CEI") (pinfunction "~{CEI}") (pintype "input"))
    (pad "22" smd roundrect (at 4.65 4.445 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "CEO") (pinfunction "~{CEO}") (pintype "input"))
    (pad "23" smd roundrect (at 4.65 5.715 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "SQW") (pinfunction "SQW") (pintype "input"))
    (pad "24" smd roundrect (at 4.65 6.985 180) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "VCC") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-24W_7.5x15.4mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "B.Cu")
    (at 130.9624 83.5152)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "nwX287.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Jumper, 3-pole, both open")
    (property "ki_keywords" "Jumper SPDT")
    (attr exclude_from_pos_files)
    (fp_text reference "JP1" (at 0 1.8 180) (layer "B.SilkS") hide)
    (fp_text value "Jumper_3_Open" (at 0 -1.9 180) (layer "B.Fab"))
    (fp_text user "Intl" (at -1.27 2.341572 90 unlocked) (layer "B.SilkS"))
    (fp_text user "Mot" (at 1.3208 2.413 90 unlocked) (layer "B.SilkS"))
    (pad "1" smd custom (at -1.3 0) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 1 "GND") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.55 -0.75)
            (xy 0 -0.75)
            (xy 0 0.75)
            (xy 0.55 0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd rect (at 0 0) (size 1 1.5) (layers "B.Cu" "B.Mask")
      (net 23 "VOUT") (pinfunction "C") (pintype "passive"))
    (pad "3" smd custom (at 1.3 0) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 2 "VCC") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 -0.75)
            (xy -0.55 -0.75)
            (xy -0.55 0.75)
            (xy 0 0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (gr_line (start 125.476 77.851) (end 133.604 77.851)
    (layer "Edge.Cuts"))
  (gr_arc (start 135.636 77.851) (mid 134.62 78.932482) (end 133.604 77.851)
    (layer "Edge.Cuts"))
  (gr_line (start 135.636 77.851) (end 143.764 77.851)
    (layer "Edge.Cuts"))
  (gr_line (start 143.764 108.966) (end 125.476 108.966)
    (layer "Edge.Cuts"))
  (gr_line (start 125.476 108.966) (end 125.476 77.851)
    (layer "Edge.Cuts"))
  (gr_line (start 143.764 77.851) (end 143.764 108.966)
    (layer "Edge.Cuts"))
  (gr_text "rev.${REVISION}" (at 138.3792 107.696) (layer "F.SilkS"))
  (gr_text "4" (at 137.668 79.629) (layer "F.SilkS"))
  (gr_text "3" (at 131.572 79.629) (layer "F.SilkS"))
  (gr_text "by Necroware" (at 134.62 85.344) (layer "F.Mask"))
  (gr_text "nwX287" (at 134.747 82.55) (layer "F.Mask"))
  (zone (net 1) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.764 108.966)
        (xy 125.476 108.966)
        (xy 125.476 77.851)
        (xy 143.764 77.851)
      )
    )
  )
)
